1. **Network bonding or teaming provide us redundancy.**
2. **If you are using only single NIC card and if it’s failed then your server won’t be accessible. So, in such scenario network bonding is important.**
3. **Here you can use 3 mechanisms namely,**

**Round Robin**

**Failed over**

**Load balancing**

1. **#teamdctl team0 state : to check your teaming configuration**